ROUND-1

1.An ideal op-amp has infinite open-loop gain. If an ideal op-amp is used in a unity-gain buffer configuration, what is the closed-loop gain?

1. 0
2. 1
3. Infinity
4. Based on the input frequency

2.The maximum power transfer theorem states that maximum power is delivered to the load when:

1. Load resistance is equal to zero
2. Load resistance is equal to source resistance
3. Load resistance is greater than source resistance
4. Load resistance is infinite

3.The electromagnetic wave that is most strongly absorbed by the Earth's atmosphere is:

1. X rays
2. Gamma rays
3. Microwaves
4. Visible light

4. For a system to work as an oscillator, the total phase shift of the loop gain must be equal to

(A) 90°

(B) 45°

(C) 270°

(D) 360°

5. A three-input NOR gate gives high O/P when \_\_\_\_\_\_.

a) One I/P is high

b) One I/P is low

c)All I/P are low

d)All I/P are high

6.A traffic signal cycles from GREEN to YELLOW, YELLOW to RED and RED to GREEN. In each cycle, GREEN is turned on for 70 seconds, YELLOW is turned on for 5 seconds and the RED is turned on for 75 seconds. This traffic light has to be implemented using a finite state machine (FSM). The only input to this FSM is a clock of 5 second period. The minimum number of flip-flops required to implement this FSM is \_\_\_\_\_\_\_

1. 5
2. 7
3. 10
4. 15

7) In ideal Differential Amplifier, if same signal is given

to both inputs, then output will be

a) Same as input

b) Double the input

c) Not equal to zero

d) Zero

8) The purpose of level shifter in Op-amp internal circuit is to

a) Adjust DC voltage

b) Increase impedance

c) Provide high gain

d) Decrease input resistance

9) The voltage gains of an amplifier without feedback and with negative feedback respectively are 100 and 20. The percentage of negative feedback would be.

a)40%

b)5%

c)20%

d)80%

10) To obtain very high I/P and O/P impedances in a feedback amplifier, the topology used is

a)voltage series

b)current series

c)voltage shunt

d)current shunt

11) What type of material is obtained when an intrinsic semiconductor is doped with pentavalent impurity?

a) N-type semiconductor

b) Extrinsic semiconductor

c) P-type semiconductor

d) Insulator

12) npn transistors are preferred over pnp transistors because they have

1. High mobility of electrons than the mobility of holes in pnp
2. Low mobility of holes
3. High mobility of holes
4. Equal to mobility of holes

13) In a star connection, how is the line voltage related to the phase voltage?

a) Equal

b) √3 times the phase voltage

c) 1/√3 times the phase voltage

d) Twice the phase voltage

14)In an HVDC transmission system, which of the following is used as a converter?

a) Transformer

b) Cycloconverter

c) Thyristor bridge

d) Chopper

15)In a purely capacitive AC circuit, the current:

a) Lags voltage by 90°

b) Leads voltage by 90°

c) Is in phase with voltage

d) Is independent of voltage

16)Which of the following is true for a DC shunt motor when the load increases?

a) The speed remains nearly constant

b) The speed increases significantly

c) The armature current decreases

d) The motor efficiency decreases

17)Consider the following statements regarding the situation at resonant frequency :

1. For a series RLC circuit, current is minimum.

2. For a series RLC circuit, voltage across C is minimum.

3. For a series RLC circuit, current is maximum.

4. For a parallel RLC circuit, total impedance is maximum.

Of the statements

(A) 1 and 2 are correct

(B) 2 and 3 are correct

(C) 3 and 4 are correct

(D) 1 and 4 are correct

18) A long-channel NMOS transistor is biased in the linear region with Vds=50 mV and is used as a resistance. Which one of the following statements is NOT correct?

A)If the device width W is increased, the resistance decreases.

B)If the threshold voltage is reduced, the resistance decreases.

C)If the device length L is increased, the resistance increases.

D)If Vgs is increased, the resistance increases.

19)A source of angular frequency 1 rad/sec has a source impedance consisting of 1 Ω resistance in series with 1 H inductance. The load that will obtain the maximum power transfer is

A)1 Ω resistance

B)1 Ω resistance in parallel with 1 H inductance

C)1 Ω resistance in series with 1 F capacitor

D)1 Ω resistance in parallel with 1 F capacitor

20) Following is a 8086 assembly language program, After execution of the program, the status of the CF and ZF flags will be

MOV AL, 00h

SUB AL, 01h

CMP AL, FFh

HLT


A)CF = 0, ZF = 0

B)CF = 0, ZF = 1

C)CF = 1, ZF = 0

D)CF = 1, ZF = 1

21)The state transition diagram for the circuit shown is



a)A


b)B

c)C

d)D

22)Two conducting spheres S1 and S2 of radii a and b (b>a) respectively, are placed far apart and connected by a long, thin conducting wire, as shown in the figure.For some charge placed on this structure, the potential and surface electric field on S1 are

Va and Ea, and that on S2 are Vb and Eb, respectively, which of the following is CORRECT?



A)Va>Vb, Ea=Eb

B)Va=Vb, Ea>Eb

C)Va>Vb, Ea<Eb

D)Va=Vb, Ea<Eb  
  
23) Which one of the following is NOT a characteristic of an ideal op-amp?

a) Infinite input impedance

b) Zero output impedance

c) Infinite bandwidth

d) Finite voltage gain

24) The output of a D flip-flop is connected to its input. A clock is applied. What is the behavior of the circuit?

a) Acts as a counter

b) Latches a value

c) Remains in logic high

d) Remains in logic low

25) If x(t) = cos(2πt) + cos(6πt), what is the Nyquist rate for this signal?

a) 1 Hz

b) 2 Hz

c) 3 Hz

d) 6 Hz

26) In a common-emitter amplifier, if the collector resistor is increased while keeping all other parameters constant, how does the voltage gain change?

1. Increases
2. Decreases
3. Remains the same
4. Becomes unpredictable

27) An ideal sawtooth voltages waveform of frequency of 500 Hz and amplitude 3 V is generated by charging a capacitor of 2 μF in every cycle. The charging requires

a)Constant voltage source of 3 V for 1 ms

b)Constant voltage source of 3 V for 2 ms

c)Constant voltage source of 1 mA for 1 ms

d)Constant voltage source of 3 mA for 2 ms

**28) You ask your op-amp to integrate a square wave. What kind of output does it sketch for you?** a) A triangle   
 b) A constant DC line  
 c) A ramp, climbing steadily  
 d) A meme about math

**29) The capacitor in an AC circuit says:  
 a) “I lead the way!”  
 b) “I lag behind inductors.”  
 c) “Voltage is just a phase, bro.”  
 d) “I resist change, slowly.”**

**30) A plane electromagnetic wave is traveling in the +z direction. Which of the following is true?  
 a) E and H fields are parallel to z  
 b) E field is in z, H is in x  
 c) E is in x, H is in y (or vice versa)  
 d) All fields go in the same direction for team spirit**